,Width##LENGTH##INCHES,Wheel DxW (in)##OTHER##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,URL##OTHER##,Total Heating Capacity##HVAC_HEATING_LOAD##BRITISH_THERMAL_UNITS_PER_HOUR,Total Cooling Capacity##HVAC_COOLING_LOAD##BRITISH_THERMAL_UNITS_PER_HOUR,S/T##OTHER##,R410A Refrigerant Charge (oz)##OTHER##,Product data url##OTHER##,Product Guid##OTHER##,Power Factor##OTHER##,Phase##OTHER##,Outside Fan Rated Load Amps##OTHER##,Outside Fan Rated HP##OTHER##,Outside Fan Nominal RPM##OTHER##,Outside Fan Diameter (in)##OTHER##,Outdoor Sound Rating (dBa)##OTHER##,Model##OTHER##,Min. Circuit Ampacity at 230V##OTHER##,Min. Circuit Ampacity at 208V##OTHER##,Material##OTHER##,Manufacturer##OTHER##,MOCP^2 at 230V##OTHER##,MOCP^2 at 208V##OTHER##,M##LENGTH##INCHES,L##LENGTH##INCHES,Keynote##OTHER##,K##LENGTH##INCHES,J##LENGTH##INCHES,Indoor Blower Rated Load Amps##OTHER##,Indoor Blower Rated HP##OTHER##,Height##LENGTH##INCHES,H##LENGTH##INCHES,Frequency##ELECTRICAL_FREQUENCY##HERTZ,Energy Efficiency Rating##OTHER##,Electric Heat @ 240V kW##OTHER##,Electric Heat @ 240V Btu/hr##OTHER##,Edition number##OTHER##,E##LENGTH##INCHES,Description##OTHER##,Depth##LENGTH##INCHES,D##LENGTH##INCHES,Compressor Rated Load Amps##OTHER##,Compressor Locked Rotor Amps##OTHER##,Clearance Depth##LENGTH##INCHES,Clearance##OTHER##,C##LENGTH##INCHES,B##LENGTH##INCHES,Assembly Code##OTHER##,Approx. Shipping Weight (lbs)##OTHER##,Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,Actual Ventilation Air Flow##HVAC_AIR_FLOW##GALLONS_US_PER_MINUTE
3MHP4-11-091*P,28.062500000000,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mhp,8600.000000000000,8600.000000000000,0.79,44,https://www.bimobject.com/en-us/magicpak/product/mhp-single-packaged-vertical-unit,d5f253a1-e221-4e0e-8c6c-fa0ebfd26edc,1,1,0.9,1/8,1100,16,73,M Series MHP4,25.5,23,Aluminum,Magic Pak,30,25,2.250000000000,0.750000000000,15700,17.062500000000,16.000000000000,2.8,1/3,43.875000000000,8.000000000000,60.000000000000,11.1,3.6,"12,284",1,18.625000000000,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",21.500000000000,6.000000000000,3.5,21,5.000000000000,1,25.250000000000,16.875000000000,D30,192,0.000000000000,350.000000000000
3MHP4-11-181*P,28.062500000000,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mhp,16200.000000000000,17000.000000000000,0.77,80,https://www.bimobject.com/en-us/magicpak/product/mhp-single-packaged-vertical-unit,d5f253a1-e221-4e0e-8c6c-fa0ebfd26edc,1,1,0.9,1/8,1125,16,73,M Series MHP4,29.1,26.6,Aluminum,Magic Pak,30,30,2.250000000000,0.750000000000,15700,19.062500000000,16.000000000000,2.8,1/3,47.875000000000,8.000000000000,60.000000000000,11,3.6,"12,284",1,20.625000000000,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",21.500000000000,6.000000000000,6.5,37.5,5.000000000000,1,27.250000000000,18.875000000000,D30,219,0.000000000000,600.000000000000
5MHP4-11-241*P,28.062500000000,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mhp,22800.000000000000,22800.000000000000,0.76,82,https://www.bimobject.com/en-us/magicpak/product/mhp-single-packaged-vertical-unit,d5f253a1-e221-4e0e-8c6c-fa0ebfd26edc,1,1,0.9,1/4,1100,18,79,M Series MHP4,40.8,37.4,Aluminum,Magic Pak,45,40,1.000000000000,0.750000000000,15700,22.437500000000,16.000000000000,4.1,1/3,55.875000000000,8.000000000000,60.000000000000,11,4.8,"16,378",1,24.625000000000,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",24.375000000000,6.000000000000,10.1,52.0,5.000000000000,1,31.250000000000,22.875000000000,D30,268,0.000000000000,800.000000000000
5MHP4-11-301*P,28.062500000000,10x8,208.000000000000,https://www.magic-pak.com/products/m-series/mhp,26200.000000000000,28200.000000000000,0.75,60,https://www.bimobject.com/en-us/magicpak/product/mhp-single-packaged-vertical-unit,d5f253a1-e221-4e0e-8c6c-fa0ebfd26edc,1,1,1.6,1/4,1100,18,79,M Series MHP4,45.2,41.9,Aluminum,Magic Pak,50,50,1.000000000000,3.750000000000,15700,22.437500000000,10.437500000000,4.1,1/2,55.875000000000,11.375000000000,60.000000000000,11,4.8,"16,378",1,24.625000000000,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",24.375000000000,6.000000000000,15.0,72.5,5.000000000000,1,31.250000000000,22.875000000000,D30,271,0.000000000000,1025.000000000000
5MHP4-11-361*P,28.062500000000,10x8,208.000000000000,https://www.magic-pak.com/products/m-series/mhp,32400.000000000000,34600.000000000000,0.75,102,https://www.bimobject.com/en-us/magicpak/product/mhp-single-packaged-vertical-unit,d5f253a1-e221-4e0e-8c6c-fa0ebfd26edc,1,1,1.6,1/4,1100,18,79,M Series MHP4,47.7,44.4,Aluminum,Magic Pak,50,50,1.000000000000,3.750000000000,15700,22.437500000000,10.437500000000,4.1,1/2,67.875000000000,11.375000000000,60.000000000000,11.3,4.8,"16,378",1,28.625000000000,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",24.375000000000,10.000000000000,14.7,75.0,5.000000000000,1,35.250000000000,26.875000000000,D30,298,0.000000000000,1200.000000000000
3MHP4-11-121*P,28.062500000000,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mhp,11400.000000000000,11999.999999999998,0.79,52,https://www.bimobject.com/en-us/magicpak/product/mhp-single-packaged-vertical-unit,d5f253a1-e221-4e0e-8c6c-fa0ebfd26edc,1,1,0.9,1/8,1125,16,73,M Series MHP4,26.7,24.2,Aluminum,Magic Pak,30,25,2.250000000000,0.750000000000,15700,17.062500000000,16.000000000000,2.8,1/3,43.875000000000,8.000000000000,60.000000000000,11,3.6,"12,284",1,18.625000000000,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",21.500000000000,6.000000000000,5,27,5.000000000000,1,25.250000000000,16.875000000000,D30,202,0.000000000000,475.000000000000
5MHP4-11-091*P,28.062500000000,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mhp,8600.000000000000,8600.000000000000,0.79,44,https://www.bimobject.com/en-us/magicpak/product/mhp-single-packaged-vertical-unit,d5f253a1-e221-4e0e-8c6c-fa0ebfd26edc,1,1,0.9,1/8,1100,16,73,M Series MHP4,31.8,28.4,Aluminum,Magic Pak,35,30,2.250000000000,0.750000000000,15700,17.062500000000,16.000000000000,2.8,1/3,43.875000000000,8.000000000000,60.000000000000,11.1,4.8,"16,378",1,18.625000000000,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",21.500000000000,6.000000000000,3.5,21,5.000000000000,1,25.250000000000,16.875000000000,D30,192,0.000000000000,350.000000000000
5MHP4-11-121*P,28.062500000000,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mhp,11400.000000000000,11999.999999999998,0.79,52,https://www.bimobject.com/en-us/magicpak/product/mhp-single-packaged-vertical-unit,d5f253a1-e221-4e0e-8c6c-fa0ebfd26edc,1,1,0.9,1/8,1125,16,73,M Series MHP4,32.9,29.6,Aluminum,Magic Pak,35,30,2.250000000000,0.750000000000,15700,17.062500000000,16.000000000000,2.8,1/3,43.875000000000,8.000000000000,60.000000000000,11,4.8,"16,378",1,18.625000000000,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",21.500000000000,6.000000000000,5,27,5.000000000000,1,25.250000000000,16.875000000000,D30,202,0.000000000000,475.000000000000
5MHP4-11-181*P,28.062500000000,9x6,208.000000000000,,16200.000000000000,17000.000000000000,0.77,80,https://www.bimobject.com/en-us/magicpak/product/mhp-single-packaged-vertical-unit,d5f253a1-e221-4e0e-8c6c-fa0ebfd26edc,1,1,0.9,1/8,1125,16,73,M Series MHP4,35.3,32.0,Aluminum,Magic Pak,40,35,2.250000000000,0.750000000000,15700,19.062500000000,16.000000000000,2.8,1/3,47.875000000000,8.000000000000,60.000000000000,11,4.8,"16,378",1,20.625000000000,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",21.500000000000,6.000000000000,6.5,37.5,5.000000000000,1,27.250000000000,18.875000000000,,219,0.000000000000,600.000000000000
7MHP4-11-181*P,28.062500000000,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mhp,16200.000000000000,17000.000000000000,0.77,80,https://www.bimobject.com/en-us/magicpak/product/mhp-single-packaged-vertical-unit,d5f253a1-e221-4e0e-8c6c-fa0ebfd26edc,1,1,0.9,1/8,1125,16,73,M Series MHP4,47.8,42.8,Aluminum,Magic Pak,50,45,2.250000000000,0.750000000000,15700,19.062500000000,16.000000000000,2.8,1/3,47.875000000000,8.000000000000,60.000000000000,11,7.2,"24,567",1,20.625000000000,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",21.500000000000,6.000000000000,6.5,37.5,5.000000000000,1,27.250000000000,18.875000000000,D30,219,0.000000000000,600.000000000000
10MHP4-11-181*P,28.062500000000,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mhp,16200.000000000000,17000.000000000000,0.77,80,https://www.bimobject.com/en-us/magicpak/product/mhp-single-packaged-vertical-unit,d5f253a1-e221-4e0e-8c6c-fa0ebfd26edc,1,1,0.9,1/8,1125,16,73,M Series MHP4,50.0,43.3,Aluminum,Magic Pak,50,45,2.250000000000,0.750000000000,15700,19.062500000000,16.000000000000,2.8,1/3,47.875000000000,8.000000000000,60.000000000000,11,9.6,"32,757",1,20.625000000000,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",21.500000000000,6.000000000000,6.5,37.5,5.000000000000,1,27.250000000000,18.875000000000,D30,219,0.000000000000,600.000000000000
7MHP4-11-241*P,28.062500000000,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mhp,22800.000000000000,22800.000000000000,0.76,82,https://www.bimobject.com/en-us/magicpak/product/mhp-single-packaged-vertical-unit,d5f253a1-e221-4e0e-8c6c-fa0ebfd26edc,1,1,0.9,1/4,1100,18,79,M Series MHP4,53.3,48.3,Aluminum,Magic Pak,60,50,1.000000000000,0.750000000000,15700,22.437500000000,16.000000000000,4.1,1/3,55.875000000000,8.000000000000,60.000000000000,11,7.2,"24,567",1,24.625000000000,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",24.375000000000,6.000000000000,10.1,52.0,5.000000000000,1,31.250000000000,22.875000000000,D30,268,0.000000000000,800.000000000000
10MHP4-11-241*P,28.062500000000,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mhp,22800.000000000000,22800.000000000000,0.76,82,https://www.bimobject.com/en-us/magicpak/product/mhp-single-packaged-vertical-unit,d5f253a1-e221-4e0e-8c6c-fa0ebfd26edc,1,1,0.9,1/4,1100,18,79,M Series MHP4,50,43.3,Aluminum,Magic Pak,50,45,1.000000000000,0.750000000000,15700,22.437500000000,16.000000000000,4.1,1/3,55.875000000000,8.000000000000,60.000000000000,11,9.6,"32,757",1,24.625000000000,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",24.375000000000,6.000000000000,10.1,52.0,5.000000000000,1,31.250000000000,22.875000000000,D30,268,0.000000000000,800.000000000000
7MHP4-11-301*P,28.062500000000,10x8,208.000000000000,https://www.magic-pak.com/products/m-series/mhp,26200.000000000000,28200.000000000000,0.75,60,https://www.bimobject.com/en-us/magicpak/product/mhp-single-packaged-vertical-unit,d5f253a1-e221-4e0e-8c6c-fa0ebfd26edc,1,1,1.6,1/4,1100,18,79,M Series MHP4,37.5,32.5,Aluminum,Magic Pak,40,35,1.000000000000,3.750000000000,15700,22.437500000000,10.437500000000,4.1,1/2,55.875000000000,11.375000000000,60.000000000000,11,7.2,"24,567",1,24.625000000000,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",24.375000000000,6.000000000000,15.0,72.5,5.000000000000,1,31.250000000000,22.875000000000,D30,271,0.000000000000,1025.000000000000
10MHP4-11-301*P,28.062500000000,10x8,208.000000000000,https://www.magic-pak.com/products/m-series/mhp,26200.000000000000,28200.000000000000,0.75,60,https://www.bimobject.com/en-us/magicpak/product/mhp-single-packaged-vertical-unit,d5f253a1-e221-4e0e-8c6c-fa0ebfd26edc,1,1,1.6,1/4,1100,18,79,M Series MHP4,50,43.3,Aluminum,Magic Pak,50,45,1.000000000000,3.750000000000,15700,22.437500000000,10.437500000000,4.1,1/2,55.875000000000,11.375000000000,60.000000000000,11,9.6,"32,757",1,24.625000000000,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",24.375000000000,6.000000000000,15.0,72.5,5.000000000000,1,31.250000000000,22.875000000000,D30,271,0.000000000000,1025.000000000000
7MHP4-11-361*P,28.062500000000,10x8,208.000000000000,https://www.magic-pak.com/products/m-series/mhp,32400.000000000000,34600.000000000000,0.75,102,https://www.bimobject.com/en-us/magicpak/product/mhp-single-packaged-vertical-unit,d5f253a1-e221-4e0e-8c6c-fa0ebfd26edc,1,1,1.6,1/4,1100,18,79,M Series MHP4,37.5,32.5,Aluminum,Magic Pak,40,35,1.000000000000,3.750000000000,15700,22.437500000000,10.437500000000,4.1,1/2,67.875000000000,11.375000000000,60.000000000000,11.3,7.2,"24,567",1,28.625000000000,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",24.375000000000,10.000000000000,14.7,75.0,5.000000000000,1,35.250000000000,26.875000000000,D30,298,0.000000000000,1200.000000000000
10MHP4-11-361*P,28.062500000000,10x8,208.000000000000,https://www.magic-pak.com/products/m-series/mhp,32400.000000000000,34600.000000000000,0.75,102,https://www.bimobject.com/en-us/magicpak/product/mhp-single-packaged-vertical-unit,d5f253a1-e221-4e0e-8c6c-fa0ebfd26edc,1,1,1.6,1/4,1100,18,79,M Series MHP4,50,43.3,Aluminum,Magic Pak,50,45,1.000000000000,3.750000000000,15700,22.437500000000,10.437500000000,4.1,1/2,67.875000000000,11.375000000000,60.000000000000,11.3,9.6,"32,757",1,28.625000000000,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",24.375000000000,10.000000000000,14.7,75.0,5.000000000000,1,35.250000000000,26.875000000000,D30,298,0.000000000000,1200.000000000000
