,Width##LENGTH##FEET,Wheel DxW (in)##OTHER##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,URL##OTHER##,Total Cooling Capacity##HVAC_COOLING_LOAD##BRITISH_THERMAL_UNITS_PER_HOUR,S/T##OTHER##,R410A Refrigerant Charge (oz)##OTHER##,Product data url##OTHER##,Product Guid##OTHER##,Power Factor##OTHER##,Phase##OTHER##,Outside Fan Rated Load Amps##OTHER##,Outside Fan Rated HP##OTHER##,Outside Fan Nominal RPM##OTHER##,Outside Fan Diameter (in)##OTHER##,Outdoor Sound Rating (dBa)##OTHER##,Model##OTHER##,Min. Circuit Ampacity at 230V##OTHER##,Min. Circuit Ampacity at 208V##OTHER##,Material##OTHER##,Manufacturer##OTHER##,MOCP^2 at 230V##OTHER##,MOCP^2 at 208V##OTHER##,M##LENGTH##FEET,L##LENGTH##FEET,Keynote##OTHER##,K##LENGTH##FEET,J##LENGTH##FEET,Indoor Blower Rated Load Amps##OTHER##,Indoor Blower Rated HP##OTHER##,Height##LENGTH##FEET,H##LENGTH##FEET,Frequency##ELECTRICAL_FREQUENCY##HERTZ,Energy Efficiency Rating##OTHER##,Electric Heat @ 240V kW##OTHER##,Electric Heat @ 240V Btu/hr##OTHER##,Edition number##OTHER##,E##LENGTH##FEET,Description##OTHER##,Depth##LENGTH##FEET,D##LENGTH##FEET,Compressor Rated Load Amps##OTHER##,Compressor Locked Rotor Amps##OTHER##,Clearance Depth##LENGTH##FEET,Clearance##OTHER##,C##LENGTH##FEET,B##LENGTH##FEET,Assembly Code##OTHER##,Approx. Shipping Weight (lbs)##OTHER##,Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,Actual Ventilation Air Flow##HVAC_AIR_FLOW##CUBIC_FEET_PER_MINUTE
0MCE4-11-091*P,2.338541666667,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mce,8600.000000000000,0.74,40,https://www.bimobject.com/en-us/magicpak/product/mce-single-packaged-vertical-unit,b4383ca7-ccef-4691-8ef7-4364faf61c1f,0,1,0.9,1/8,1125,16,73,M Series MCE4,6.3,6.3,Aluminum,Magic Pak,15,15,0.187500000000,0.062500000000,15700,1.421875000000,1.333333333333,2.8,1/3,3.656250000000,0.666666666667,60.000000000000,11.3,N/A,N/A,1,1.552083333333,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",1.791666666667,0.500000000000,3.5,21,0.416666666667,1,2.104166666667,1.406250000000,D30,185,0.000000000000,350.000000000000
0MCE4-11-181*P,2.338541666667,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mce,17100.000000000000,0.76,60,https://www.bimobject.com/en-us/magicpak/product/mce-single-packaged-vertical-unit,b4383ca7-ccef-4691-8ef7-4364faf61c1f,0,1,0.9,1/8,1125,16,73,M Series MCE4,10.3,10.3,Aluminum,Magic Pak,15,15,0.187500000000,0.062500000000,15700,1.421875000000,1.333333333333,2.8,1/3,3.656250000000,0.666666666667,60.000000000000,11,N/A,N/A,1,1.552083333333,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",1.791666666667,0.500000000000,6.5,37.5,0.416666666667,1,2.104166666667,1.406250000000,D30,207,0.000000000000,650.000000000000
0MCE4-11-241*P,2.338541666667,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mce,22800.000000000000,0.75,76,https://www.bimobject.com/en-us/magicpak/product/mce-single-packaged-vertical-unit,b4383ca7-ccef-4691-8ef7-4364faf61c1f,0,1,0.9,1/8,1050,18,75,M Series MCE4,13.1,13.1,Aluminum,Magic Pak,20,20,0.218750000000,0.062500000000,15700,1.588541666667,1.333333333333,2.8,1/3,3.989583333333,0.666666666667,60.000000000000,11.1,N/A,N/A,1,1.718750000000,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",2.031250000000,0.500000000000,8.4,38,0.416666666667,1,2.270833333333,1.572916666667,D30,230,0.000000000000,800.000000000000
0MCE4-11-301*P,2.338541666667,10x8,208.000000000000,https://www.magic-pak.com/products/m-series/mce,28400.000000000000,0.75,79,https://www.bimobject.com/en-us/magicpak/product/mce-single-packaged-vertical-unit,b4383ca7-ccef-4691-8ef7-4364faf61c1f,0,1,1.6,1/4,1100,18,79,M Series MCE4,19.8,19.8,Aluminum,Magic Pak,30,30,0.083333333333,0.312500000000,15700,1.869791666667,0.869791666667,4.1,1/2,4.656250000000,0.947916666667,60.000000000000,11,N/A,N/A,1,2.052083333333,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",2.031250000000,0.500000000000,15,72.5,0.416666666667,1,2.604166666667,1.906250000000,D30,256,0.000000000000,1000.000000000000
0MCE4-11-361*P,2.338541666667,10x8,208.000000000000,https://www.magic-pak.com/products/m-series/mce,34600.000000000000,0.73,94,https://www.bimobject.com/en-us/magicpak/product/mce-single-packaged-vertical-unit,b4383ca7-ccef-4691-8ef7-4364faf61c1f,0,1,1.6,1/4,1100,18,79,M Series MCE4,21.8,21.8,Aluminum,Magic Pak,35,35,0.083333333333,0.312500000000,15700,1.869791666667,0.869791666667,4.1,1/2,5.656250000000,0.947916666667,60.000000000000,11.3,N/A,N/A,1,2.385416666667,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",2.031250000000,0.833333333333,14.7,75,0.416666666667,1,2.937500000000,2.239583333333,,286,0.000000000000,1200.000000000000
0MCE4-11-121*P,2.338541666667,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mce,11999.999999999998,0.71,47,https://www.bimobject.com/en-us/magicpak/product/mce-single-packaged-vertical-unit,b4383ca7-ccef-4691-8ef7-4364faf61c1f,0,1,0.9,1/8,1125,16,73,M Series MCE4,7.6,7.6,Aluminum,Magic Pak,15,15,0.187500000000,0.062500000000,15700,1.421875000000,1.333333333333,2.8,1/3,3.656250000000,0.666666666667,60.000000000000,11.3,N/A,N/A,1,1.552083333333,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",1.791666666667,0.500000000000,5,27,0.416666666667,1,2.104166666667,1.406250000000,D30,193,0.000000000000,400.000000000000
3MCE4-11-091*P,2.338541666667,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mce,8600.000000000000,0.74,40,https://www.bimobject.com/en-us/magicpak/product/mce-single-packaged-vertical-unit,b4383ca7-ccef-4691-8ef7-4364faf61c1f,0,1,0.9,1/8,1125,16,73,M Series MCE4,19.5,17,Aluminum,Magic Pak,20,20,0.187500000000,0.062500000000,15700,1.421875000000,1.333333333333,2.8,1/3,3.656250000000,0.666666666667,60.000000000000,11.3,3.6,12.284,1,1.552083333333,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",1.791666666667,0.500000000000,3.5,21,0.416666666667,1,2.104166666667,1.406250000000,D30,185,0.000000000000,350.000000000000
5MCE4-11-091*P,2.338541666667,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mce,8600.000000000000,0.74,40,https://www.bimobject.com/en-us/magicpak/product/mce-single-packaged-vertical-unit,b4383ca7-ccef-4691-8ef7-4364faf61c1f,0,1,0.9,1/8,1125,16,73,M Series MCE4,26.3,22.9,Aluminum,Magic Pak,30,25,0.187500000000,0.062500000000,15700,1.421875000000,1.333333333333,2.8,1/3,3.656250000000,0.666666666667,60.000000000000,11.3,4.8,16.378,1,1.552083333333,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",1.791666666667,0.500000000000,3.5,21,0.416666666667,1,2.104166666667,1.406250000000,D30,185,0.000000000000,350.000000000000
3MCE4-11-121*P,2.338541666667,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mce,11999.999999999998,0.71,47,https://www.bimobject.com/en-us/magicpak/product/mce-single-packaged-vertical-unit,b4383ca7-ccef-4691-8ef7-4364faf61c1f,0,1,0.9,1/8,1125,16,73,M Series MCE4,19.5,17,Aluminum,Magic Pak,20,20,0.187500000000,0.062500000000,15700,1.421875000000,1.333333333333,2.8,1/3,3.656250000000,0.666666666667,60.000000000000,11.3,3.6,12.284,1,1.552083333333,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",1.791666666667,0.500000000000,5,27,0.416666666667,1,2.104166666667,1.406250000000,D30,193,0.000000000000,400.000000000000
5MCE4-11-121*P,2.338541666667,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mce,11999.999999999998,0.71,47,https://www.bimobject.com/en-us/magicpak/product/mce-single-packaged-vertical-unit,b4383ca7-ccef-4691-8ef7-4364faf61c1f,0,1,0.9,1/8,1125,16,73,M Series MCE4,26.3,22.9,Aluminum,Magic Pak,30,25,0.187500000000,0.062500000000,15700,1.421875000000,1.333333333333,2.8,1/3,3.656250000000,0.666666666667,60.000000000000,11.3,4.8,16.378,1,1.552083333333,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",1.791666666667,0.500000000000,5,27,0.416666666667,1,2.104166666667,1.406250000000,D30,193,0.000000000000,400.000000000000
3MCE4-11-181*P,2.338541666667,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mce,17100.000000000000,0.76,60,https://www.bimobject.com/en-us/magicpak/product/mce-single-packaged-vertical-unit,b4383ca7-ccef-4691-8ef7-4364faf61c1f,0,1,0.9,1/8,1125,16,73,M Series MCE4,19.5,17,Aluminum,Magic Pak,20,20,0.187500000000,0.062500000000,15700,1.421875000000,1.333333333333,2.8,1/3,3.656250000000,0.666666666667,60.000000000000,11,3.6,12.284,1,1.552083333333,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",1.791666666667,0.500000000000,6.5,37.5,0.416666666667,1,2.104166666667,1.406250000000,D30,207,0.000000000000,650.000000000000
5MCE4-11-181*P,2.338541666667,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mce,17100.000000000000,0.76,60,https://www.bimobject.com/en-us/magicpak/product/mce-single-packaged-vertical-unit,b4383ca7-ccef-4691-8ef7-4364faf61c1f,0,1,0.9,1/8,1125,16,73,M Series MCE4,26.3,22.9,Aluminum,Magic Pak,30,25,0.187500000000,0.062500000000,15700,1.421875000000,1.333333333333,2.8,1/3,3.656250000000,0.666666666667,60.000000000000,11,4.8,16.378,1,1.552083333333,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",1.791666666667,0.500000000000,6.5,37.5,0.416666666667,1,2.104166666667,1.406250000000,D30,207,0.000000000000,650.000000000000
7MCE4-11-181*P,2.338541666667,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mce,17100.000000000000,0.76,60,https://www.bimobject.com/en-us/magicpak/product/mce-single-packaged-vertical-unit,b4383ca7-ccef-4691-8ef7-4364faf61c1f,0,1,0.9,1/8,1125,16,73,M Series MCE4,39.3,34.3,Aluminum,Magic Pak,40,35,0.187500000000,0.062500000000,15700,1.421875000000,1.333333333333,2.8,1/3,3.656250000000,0.666666666667,60.000000000000,11,7.2,24.567,1,1.552083333333,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",1.791666666667,0.500000000000,6.5,37.5,0.416666666667,1,2.104166666667,1.406250000000,D30,207,0.000000000000,650.000000000000
10MCE4-11-181*P,2.338541666667,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mce,17100.000000000000,0.76,60,https://www.bimobject.com/en-us/magicpak/product/mce-single-packaged-vertical-unit,b4383ca7-ccef-4691-8ef7-4364faf61c1f,0,1,0.9,1/8,1125,16,73,M Series MCE4,52.1,45.5,Aluminum,Magic Pak,60,50,0.187500000000,0.062500000000,15700,1.421875000000,1.333333333333,2.8,1/3,3.656250000000,0.666666666667,60.000000000000,11,9.6,32.757,1,1.552083333333,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",1.791666666667,0.500000000000,6.5,37.5,0.416666666667,1,2.104166666667,1.406250000000,D30,207,0.000000000000,650.000000000000
5MCE4-11-241*P,2.338541666667,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mce,22800.000000000000,0.75,76,https://www.bimobject.com/en-us/magicpak/product/mce-single-packaged-vertical-unit,b4383ca7-ccef-4691-8ef7-4364faf61c1f,0,1,0.9,1/8,1050,18,75,M Series MCE4,26.3,22.9,Aluminum,Magic Pak,30,25,0.218750000000,0.062500000000,15700,1.588541666667,1.333333333333,2.8,1/3,3.989583333333,0.666666666667,60.000000000000,11.1,4.8,16.378,1,1.718750000000,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",2.031250000000,0.500000000000,8.4,38,0.416666666667,1,2.270833333333,1.572916666667,D30,230,0.000000000000,800.000000000000
7MCE4-11-241*P,2.338541666667,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mce,22800.000000000000,0.75,76,https://www.bimobject.com/en-us/magicpak/product/mce-single-packaged-vertical-unit,b4383ca7-ccef-4691-8ef7-4364faf61c1f,0,1,0.9,1/8,1050,18,75,M Series MCE4,39.8,34.8,Aluminum,Magic Pak,40,35,0.218750000000,0.062500000000,15700,1.588541666667,1.333333333333,2.8,1/3,3.989583333333,0.666666666667,60.000000000000,11.1,7.2,24.567,1,1.718750000000,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",2.031250000000,0.500000000000,8.4,38,0.416666666667,1,2.270833333333,1.572916666667,D30,230,0.000000000000,800.000000000000
10MCE4-11-241*P,2.338541666667,9x6,208.000000000000,https://www.magic-pak.com/products/m-series/mce,22800.000000000000,0.75,76,https://www.bimobject.com/en-us/magicpak/product/mce-single-packaged-vertical-unit,b4383ca7-ccef-4691-8ef7-4364faf61c1f,0,1,0.9,1/8,1050,18,75,M Series MCE4,52.9,46.2,Aluminum,Magic Pak,60,50,0.218750000000,0.062500000000,15700,1.588541666667,1.333333333333,2.8,1/3,3.989583333333,0.666666666667,60.000000000000,11.1,9.6,32.757,1,1.718750000000,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",2.031250000000,0.500000000000,8.4,38,0.416666666667,1,2.270833333333,1.572916666667,D30,230,0.000000000000,800.000000000000
5MCE4-11-301*P,2.338541666667,10x8,208.000000000000,https://www.magic-pak.com/products/m-series/mce,28400.000000000000,0.75,79,https://www.bimobject.com/en-us/magicpak/product/mce-single-packaged-vertical-unit,b4383ca7-ccef-4691-8ef7-4364faf61c1f,0,1,1.6,1/4,1100,18,79,M Series MCE4,26.3,22.9,Aluminum,Magic Pak,30,30,0.083333333333,0.312500000000,15700,1.869791666667,0.869791666667,4.1,1/2,4.656250000000,0.947916666667,60.000000000000,11,4.8,16.378,1,2.052083333333,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",2.031250000000,0.500000000000,15,72.5,0.416666666667,1,2.604166666667,1.906250000000,D30,256,0.000000000000,1000.000000000000
7MCE4-11-301*P,2.338541666667,10x8,208.000000000000,https://www.magic-pak.com/products/m-series/mce,28400.000000000000,0.75,79,https://www.bimobject.com/en-us/magicpak/product/mce-single-packaged-vertical-unit,b4383ca7-ccef-4691-8ef7-4364faf61c1f,0,1,1.6,1/4,1100,18,79,M Series MCE4,39,34,Aluminum,Magic Pak,40,35,0.083333333333,0.312500000000,15700,1.869791666667,0.869791666667,4.1,1/2,4.656250000000,0.947916666667,60.000000000000,11,7.2,24.567,1,2.052083333333,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",2.031250000000,0.500000000000,15,72.5,0.416666666667,1,2.604166666667,1.906250000000,D30,256,0.000000000000,1000.000000000000
10MCE4-11-301*P,2.338541666667,10x8,208.000000000000,https://www.magic-pak.com/products/m-series/mce,28400.000000000000,0.75,79,https://www.bimobject.com/en-us/magicpak/product/mce-single-packaged-vertical-unit,b4383ca7-ccef-4691-8ef7-4364faf61c1f,0,1,1.6,1/4,1100,18,79,M Series MCE4,52.9,45.2,Aluminum,Magic Pak,60,50,0.083333333333,0.312500000000,15700,1.869791666667,0.869791666667,4.1,1/2,4.656250000000,0.947916666667,60.000000000000,11,9.6,32.757,1,2.052083333333,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",2.031250000000,0.500000000000,15,72.5,0.416666666667,1,2.604166666667,1.906250000000,D30,256,0.000000000000,1000.000000000000
5MCE4-11-361*P,2.338541666667,10x8,208.000000000000,https://www.magic-pak.com/products/m-series/mce,34600.000000000000,0.73,94,https://www.bimobject.com/en-us/magicpak/product/mce-single-packaged-vertical-unit,b4383ca7-ccef-4691-8ef7-4364faf61c1f,0,1,1.6,1/4,1100,18,79,M Series MCE4,26.3,22.9,Aluminum,Magic Pak,35,35,0.083333333333,0.312500000000,15700,1.869791666667,0.869791666667,4.1,1/2,5.656250000000,0.947916666667,60.000000000000,11.3,4.8,16.378,1,2.385416666667,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",2.031250000000,0.833333333333,14.7,75,0.416666666667,1,2.937500000000,2.239583333333,D30,286,0.000000000000,1200.000000000000
7MCE4-11-361*P,2.338541666667,10x8,208.000000000000,https://www.magic-pak.com/products/m-series/mce,34600.000000000000,0.73,94,https://www.bimobject.com/en-us/magicpak/product/mce-single-packaged-vertical-unit,b4383ca7-ccef-4691-8ef7-4364faf61c1f,0,1,1.6,1/4,1100,18,79,M Series MCE4,39.1,34.1,Aluminum,Magic Pak,40,35,0.083333333333,0.312500000000,15700,1.869791666667,0.869791666667,4.1,1/2,5.656250000000,0.947916666667,60.000000000000,11.3,7.2,24.567,1,2.385416666667,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",2.031250000000,0.833333333333,14.7,75,0.416666666667,1,2.937500000000,2.239583333333,D30,286,0.000000000000,1200.000000000000
10MCE4-11-361*P,2.338541666667,10x8,208.000000000000,https://www.magic-pak.com/products/m-series/mce,34600.000000000000,0.73,94,https://www.bimobject.com/en-us/magicpak/product/mce-single-packaged-vertical-unit,b4383ca7-ccef-4691-8ef7-4364faf61c1f,0,1,1.6,1/4,1100,18,79,M Series MCE4,52.3,45.6,Aluminum,Magic Pak,60,50,0.083333333333,0.312500000000,15700,1.869791666667,0.869791666667,4.1,1/2,5.656250000000,0.947916666667,60.000000000000,11.3,9.6,32.757,1,2.385416666667,"MagicPak's M-Series Units all-in-one design means engineers no longer need to specify many of the other parts that come along with traditional split-system heating and cooling solutions. Chaseways aren't needed, nor are basepads, external utility connections, disconnects or allowances for refrigerant lines. MagicPak's M-Series Units offer consistency from room to room and floor to floor, so specification is the same and installation time is shortened.",2.031250000000,0.833333333333,14.7,75,0.416666666667,1,2.937500000000,2.239583333333,D30,286,0.000000000000,1200.000000000000
